You are here: File Descriptions > Resource Manager > OSTM - Temporary CONFIG.BBX Master

# OSTM - Temporary CONFIG.BBX Master

The Temporary CONFIG.BBX Master file stores a master list of devices found in the CONFIG.BBX file. This file is built and removed during the Devices function in Resource Manager.

| Template: |
| IOLIST: | 0999 OSTM: IOLIST TM0$, TM1$, TM2$, TM3$, TM4$
| String Sizes: | DIM TM0$(4), TM1$(1), TM2$(4), TM3$(74), TM4$(25)

Key Definitions

| Key Number | Field | Description
| 0 | [1:1:4] | Sequence Number
| 1 | [2:1:1] + | Record Type +
|  | [1:1:4] | Sequence Number
|  | __________ |
|  | 3 segments |

Temporary CONFIG.BBX Master

| File Name: | OSTM | Record Size: | 113(128)
| File Type: | Mkeyed - Dynamic | Number of Keys: | 2

| Field | Field Name | Variable | Description | A/N | Length | Note
| 1 | SEQ | TM0$ | Sequence Number | A | 4 | "0000"
| 2 | RTYP | TM1$ | Record Type | A | 1 | T = Terminal
|  |  |  |  |  |  | P = Printer
|  |  |  |  |  |  | D = Plotter
|  |  |  |  |  |  | O = Other
|  |  |  |  |  |  | I = If statement
| 3 | DEVID | TM2$ | Device ID | A | 4 |
| 4 | LINEDTA | TM3$ | Line Data | A | 74 |
| 5 | USRID | TM4$ | User ID | A | 25 |